Product Specification Guide
Vari-Green Control – Indoor Air Quality – VOC (Volatile Organic Compound)

Control to be a packaged Indoor Air Quality control designed to regulate fan speed based on level of VOC concentration in a space.  Control shall include a Proportional Integral Derivative (PID) feedback loop and shall have labeled terminal strips for easy wiring.  Fan shall be direct drive including an electronic commutation (EC) Vari-Green motor. Control package shall be Vari-Green Indoor Air Quality – VOC Control.