Title: Microsoft Word - Series CC5F.docx
Author: bshaloo
Last saved by: Schultz, Sue

Series XG-CC5F – Specifications
Cube Core Return Filter Grille

XG-CC5F-1 Surface Mount 
XG-CC5F-6 T-bar Lay-in
XG-CC5F-9 Donn Fineline T-bar

Air Inlets shall be model XG-CC5F with a 1/2" x 1/2" x 1/2" cubed core manufactured by GREENHECK.  Border shall be 1 1/4" wide. Units shall be filter return or exhaust grilles of aluminum construction and with an extruded aluminum border and an aluminum cubed core. 

Units shall include a hinged face and integral frame designed to accept a 1" (2” or 4” optional) thick filter. Filters are to be provided by others.  Filter face shall be secured in place with 1/4" turn fasteners. 

The units shall be the size and quantity as outlined in the plans and specifications.

For Surface mounting:
Units shall be designed for surface mounting applications and be provided with counter sunk screw holes on the face of the device.

For T-Bar Lay-in:
Units shall be designed to integrate into the specified ceiling system. 

Damper Accessories (Optional)
Optional opposed blade damper shall be constructed of steel (model XG-OBD) or aluminum (model XG-OBDA). Damper must be operable from the face of the diffuser.

Performance Specification
The manufacturer shall provide published performance data. Data shall be tested in accordance to ANSI/ASHRAE Standard 70- 2006

Paint Specification
Process shall be anodic electrodeposition using an anodic acrylic paint. Units shall undergo pre‐ treatment including a pressurized spray stage using an alkaline cleaner and a de‐ionized water rinse.

Copyright © 2021 Greenheck Fan Corporation		Page  of 
April 2021