Product Specification Guide
Auto-Cleaning Needlepoint Bipolar Ionization (NPBI®) With AMPLIFY™ Overhead Fans

Note to User: This document is subject to copyright protection and is proprietary to Greenheck Fan Corporation. However, Greenheck Fan Corporation authorizes the user a limited non-exclusive license to use this document or portions of it for the purpose of preparing written product specifications for the appropriate CSI MasterFormat category. All information in this document as provided by Greenheck Fan Corporation is informational in nature and is provided without representation or warranty of any kind as to the user or any other party, including, without limitation, ANY IMPLIED WARRANTY OF MERCHANTABILITY, FITNESS FOR PARTICULAR PURPOSE, OR NON-INFRINGEMENT. To the greatest extent permitted by applicable law, Greenheck Fan Corporation assumes no liability, and User assumes all liability and risk, for the use or results from the use of this document or the information contained herein, whether as modified by the user or not. Users should consult www.greenheck.com to verify that this document represents the most current version. 

*************************************************************************************************************
Specifier Notes: This product specification guide must be carefully reviewed and edited by the Engineer to meet the requirements of the project and local building code. Coordinate with other specification sections and the drawings.

Delete all unnecessary “Specifier Notes” when editing this section.
*************************************************************************************************************
The needlepoint bipolar ionization (NPBI®) system shall include auto-cleaning carbon fiber brush emitters. Input voltage must be universal 24VAC to 240VAC. The system shall include a programmable auto-cleaning cycle, operation status LED, and integral Building Management System (BMS) alarm contacts. The system shall be capable of producing >300 million positive and negative ions per cc/sec. 

The needlepoint bipolar ionization system shall be UL 2998 listed which validates that the electronic air cleaner has no ozone emission, as ozone can be potentially harmful to human health.

The needlepoint bipolar ionization system shall be provided by Greenheck to integrate and function with AMPLIFY™ overhead fans as tested.

Due to continuous research, Greenheck reserves the right to change specifications 
without notice.