Series XG-CC45 – Specifications

Return Grilles – Sightproof Cubed Core – Aluminum
XG-CC45-1 – Surface Mount 
XG-CC45-6 – T-bar Lay-in
XG-CC45 TBC-6 – T-bar Lay-in Core Only 
XG-CC45-7 – Concealed Spline
XG-CC45-8 – Tegular T-bar 
XG-CC45-9 – Donn Fineline

Air inlets shall be model XG-CC45.

Model XG-CC45 shall be manufactured by GREENHECK. XG-CC45 shall be a 1/2" x 1/2" x 1/2" cubed core with 45-degree deflection angle. Border shall be 1 1/4" wide. Units shall be return or exhaust grilles of aluminum construction and with an extruded aluminum border and an aluminum cubed core. Units shall use a sight-proof cubed core with 45 degree deflection angle. The units shall be the size and quantity as outlined in the plans and specifications. Units shall be designed to integrate into the specified ceiling system.

Damper Accessories (Optional)
Optional opposed blade damper shall be constructed of steel (Model XG-OBD) or aluminum (Model XG-OBDA). Damper must be operable from the face of the diffuser.

Performance Specification
The manufacturer shall provide published performance data. Data shall be tested in accordance to ANSI/ASHRAE Standard 70-2006