Series XG-RP – Specifications

Air Inlets shall be model XG-RP manufactured by GREENHECK. Units shall be perforated face, return or exhaust grilles constructed of aluminum.

Perforate face shall have 3/16" diameter holes on 1/4" centers and shall have a 51% free area. The units shall be the size and quantity as outlined in the plans and specifications.

Border shall be 1 1/4". Units shall be designed for surface mounting applications and be provided with counter sunk screw holes on the face of the device.

Damper Accessories (Optional)
Optional opposed blade damper shall be constructed of steel (Model XG-OBD) or aluminum (Model XG-OBDA). Damper must be operable from the face of the diffuser.

Performance Specification
The manufacturer shall provide published performance data. Data shall be tested in accordance to ANSI/ASHRAE Standard 70- 2006.