Title: Microsoft Word - Series 4100.docx
Author: bshaloo
Last saved by: Schultz, Sue

Series XG-4100/XG-4200/XG-4300 – Specifications

Supply - Single Deflection Supply Grilles and Registers – Aluminum/Series 

XG-4152 – 4 3/8" deep collars with 1 1/2" blades on 1 1/2" centers
XG- 4252 – 1 7/8" deep collars with 1 1/2" blades on 1 1/2" centers 
XG-4352 – 7" deep collars with 3" blades on 3" centers

Air Outlets shall be Greenheck XG-V4152, XG-V4252, or XG-V4352 with vertical front blades or 
XG-4152, XG-H4252, or XG-H4352 with horizontal front blades manufactured by GREENHECK Units shall be single deflection supply grilles of extruded aluminum construction.

Options
Outlets shall have 4 3/8" deep collars with 1 1/2" blades on 1 1/2" centers Outlets shall have 1 7/8" deep collars with 1 1/2" blades on 1 1/2" centers Outlets shall have 7" deep collars with 3" blades on 3" centers

Options
Units shall include an Inverted Frame Units shall include a Trunk Latch Frame.

The units shall be the size and quantity as outlined in the plans and specifications.
Border shall be 1 1/2" wide with individually adjustable, aerodynamically shaped deflector blades. Units shall be designed for surface mounting applications and be provided with screw holes on the face of the device.

Blades shall pivot in friction mounting retainers. Retainers shall hold the deflector blade position throughout the specified operating range of the device. Metal friction wires are not acceptable.

Optional Damper
Optional opposed blade damper shall be constructed of steel (model XG-OBD) or aluminum (model XG-OBDA). Damper must be operable from the face of the diffuser.

Supply - Double Deflection Supply Grilles and Registers – Aluminum/Series 

XG-4154 – 4 3/8" deep collars with 1 1/2" blades on 1 1/2" centers
XG-4254 – 1 7/8" deep collars with 1 1/2" blades on 1 1/2" centers 
XG-4354 – 7" deep collars with 3" blades on 3" centers

Air Outlets shall be Greenheck XG-V4154, XG-V4254, or XG-V4354 with vertical front blades or 
XG-H4154, XG-H4254, or XG-H4354 with horizontal front blades manufactured by GREENHECK. Units shall be single deflection supply grilles with front and rear sets of deflection extruded aluminum blades.

Options
Outlets shall have 4 3/8" deep collars with 1 1/2" blades on 1 1/2" centers Outlets shall have 1 7/8" deep collars with 1 1/2" blades on 1 1/2" centers Outlets shall have 7" deep collars with 3" blades on 3" centers.

Copyright © 2022 Greenheck Fan Corporation		Page  of 
October 2022