Series XG-SGRH – Specifications

Air outlets shall be model XG-SG-RH manufactured by GREENHECK. Units shall be minimum security supply grilles of steel construction. Units shall have 14 gauge horizontal fixed louvers set at 0° (or 40°) on 1/2" centers. Louvers shall be reinforced and welded to a steel sleeve. Units shall include a 14 gauge steel face plate and a 10 gauge by #2 wire mesh screen located behind the louvers and secured by 1/8" welded angle. Units shall include a 1 1/2" border.

The units shall be the size and quantity as outline in the plans and specifications.

Optional opposed blade damper shall be constructed of steel (model XG-OBD) or aluminum (model XG-OBDA). Damper must be operable from the face of the diffuser.

Performance Specification
The manufacturer shall provide published performance data. Data shall be tested in accordance to ANSI/ASHRAE Standard 70- 2006