Series XG-SGWM – Specifications

Maximum Security Supply Grilles – 

XG-SGWM with Woven Mesh

XG-SGWM - Steel

XG-SGWM - Stainless Steel

Air diffusers shall be model XG-SGWM manufactured by GREENHECK. Units shall be medium security grilles of steel construction with a face plate constructed of 12-gauge steel backed by a 10-gauge woven mesh screen. The face shall be stitch welded to the 12-gauge sleeve. Units shall have a 1" border.
The units shall be the size and quantity as outlined in the plans and specifications. Optional opposed blade damper shall be constructed of steel (model XG-OBD).

Rear operation of the damper is recommended.

Performance Specification
The manufacturer shall provide published performance data. Data shall be tested in accordance to ANSI/ ASHRAE Standard 70-2006.

Paint Specification
Process shall be anodic electro-deposition using an anodic acrylic paint. Units shall undergo pre-treatment including a pressurized spray stage using an alkaline cleaner and a de-ionized water rinse.